

#################### PYOTE 5.7.11  session started: Fri Oct  3 17:01:20 2025  ####################

filename: C:/Users/Stefan/Pictures/2025/2025-10-02 Sternbed/4 - (68988) 2002 TU34/lc-21.csv

==================== file header lines ====================
# PyMovie Version 4.1.5
# source: C:\Users\Stefan\Pictures\2025\2025-10-02 Sternbed\4 - (68988) 2002 TU34\20251003_040441_816x620_G24dB_0040ms.adv
#
# Aperture photometry was used to extract the lightcurves
#
# lunar background: False
# yellow mask = default: False
#
# aperture name: target
# ____ aperture size: 21
# ____ x,y: (398, 264) at frame 749
# ____ threshold: 289
# ____ def mask radius: 4.0
# ____ color: green
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 9
#
# aperture name: ref
# ____ aperture size: 21
# ____ x,y: (249, 329) at frame 749
# ____ threshold: 120
# ____ def mask radius: 4.0
# ____ color: red
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 10
#
# aperture name: track
# ____ aperture size: 21
# ____ x,y: (384, 536) at frame 749
# ____ threshold: 706
# ____ def mask radius: 4.0
# ____ color: yellow
# ____ joggable: True
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 11
#
# date at frame 0: 2025-10-03
#ACQUISITION-DELAY: 0.0
#ALTITUDE: 552.0
#AUTHOR: Stefan Meister
#BINNING-X: 2
#BINNING-Y: 2
#CAMERA-DRIVER-NAME: UVC
#CAMERA-FIRMWARE-VERSION: 1.3.3
#CAMERA-MODEL: DVTI+CAM
#CAMERA-SENSOR-INFO: Sony IMX430LLJ-C (9.2mm 1624x1240 4.5um CIS)
#CAMERA-SERIAL-NO: 17
#CAMERA-VENDOR-NAME: DVTI
#COMMENT: 
#HEIGHT: 620
#INSTRUMENT: DVTI+CAM #17 FW 1.3.3, Sensor IMX430
#LATITUDE: 47.5195784
#LONGITUDE: 8.5706952
#OBJNAME: (68988) 2002 TU34 occ. UCAC4 545-045150
#OBSERVER: Stefan Meister
#RECORDER-SOFTWARE: DvtiCamControl
#RECORDER-SOFTWARE-VERSION: 5.9.0-81
#TELESCOPE: Newton 2.5m
#WIDTH: 816
#
# Aperture photometry was used to extract the lightcurves
==================== end header lines ====================

No time step irregularities found.

timeDelta: 0.0399893 seconds per reading
timestamp error rate: 0.00%

Use min/max event to locate a "D and R" event has been selected

minEvent: 2  maxEvent: 8

Number of candidate solutions: 5201 (using event min/max entries)

New solver results...

Integer (non-subframe) solution...
B:6533.15  A:753.80
in entryNum units: D: 367  R: 372

noise corr coefs: [1.00]  (based on 744 points)  sigmaB: 1024.55

noise corr coefs: [1.00]  (based on 744 points)  sigmaB: 1024.55

Subframe adjusted solution...
B:6533.15  A:372.75
in entryNum units: D: 367  R: 371  D(subframe): 367.0000  R(subframe): 371.7363

in frameNum units: D: 368  R: 372  D(subframe): 368.0000  R(subframe): 372.7363

... end New solver results

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1234
hiDbar   @ .68 ci:   0.1388
loDbar   @ .95 ci:  -0.3142
hiDbar   @ .95 ci:   0.2833
loDbar   @ .9973 ci:  -0.6113
hiDbar   @ .9973 ci:   0.5817

loDurBar @ .68 ci:  -0.1891
hiDurBar @ .68 ci:   0.1989
loDurBar @ .95 ci:  -0.4192
hiDurBar @ .95 ci:   0.4232
loDurBar @ .9973 ci:  -0.7450
hiDurBar @ .9973 ci:   0.7521

Timestamp validity check ...

From timestamps at D and R, calculated 4 reading blocks.  From reading blocks, calculated 4 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 6533.15  {+/- 37.58}  sigmaB: 1024.55

A: 372.75  {+/- 272.98}  sigmaA: 527.66

magDrop report: percentDrop: 94.3  magDrop: 3.109  +/- 0.795  (0.68 ci)

DNR: 6.01

D: 368.00 {+0.14,-0.12} (frame number)
D: [04:04:55.9310]  {+0.0056,-0.0049} seconds

R: 372.74 {+0.12,-0.14} (frame number)
R: [04:04:56.1204]  {+0.0049,-0.0056} seconds

Duration (R - D): 4.7363 {+0.1940,-0.1940} readings
Duration (R - D): 0.1894 {+0.0078,-0.0078} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 6533.15  {+/- 75.16}  sigmaB: 1024.55

A: 372.75  {+/- 545.97}  sigmaA: 527.66

magDrop report: percentDrop: 94.3  magDrop: 3.109  +/- 1.590  (0.95 ci)

DNR: 6.01

D: 368.00 {+0.28,-0.31} (frame number)
D: [04:04:55.9310]  {+0.0113,-0.0126} seconds

R: 372.74 {+0.31,-0.28} (frame number)
R: [04:04:56.1204]  {+0.0126,-0.0113} seconds

Duration (R - D): 4.7363 {+0.4212,-0.4212} readings
Duration (R - D): 0.1894 {+0.0168,-0.0168} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 6533.15  {+/- 112.74}  sigmaB: 1024.55

A: 372.75  {+/- 818.95}  sigmaA: 527.66

magDrop report: percentDrop: 94.3  magDrop: 3.109  +/- 2.385  (0.9973 ci)

DNR: 6.01

D: 368.00 {+0.58,-0.61} (frame number)
D: [04:04:55.9310]  {+0.0233,-0.0244} seconds

R: 372.74 {+0.61,-0.58} (frame number)
R: [04:04:56.1204]  {+0.0244,-0.0233} seconds

Duration (R - D): 4.7363 {+0.7485,-0.7485} readings
Duration (R - D): 0.1894 {+0.0299,-0.0299} seconds

=============== end 0.9973 containment interval report =============

D frame number: 368.00
D: 0.6800 containment intervals:  {+/- 0.14} (readings)
D: 0.9500 containment intervals:  {+/- 0.31} (readings)
D: 0.9973 containment intervals:  {+/- 0.61} (readings)

R frame number: 372.74
R: 0.6800 containment intervals:  {+/- 0.14} (readings)
R: 0.9500 containment intervals:  {+/- 0.31} (readings)
R: 0.9973 containment intervals:  {+/- 0.61} (readings)

Duration (R - D): 4.7363 readings
Duration: 0.6800 containment intervals:  {+/- 0.1940} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.4212} (readings)
Duration: 0.9973 containment intervals:  {+/- 0.7485} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.


The observed drop has an estimated 13.3 sigma level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 94.3  magDrop: 3.109  +/- 1.590  (0.95 ci)

DNR: 6.01

D time: [04:04:55.9310]
D: 0.6800 containment intervals:  {+/- 0.0056} seconds
D: 0.9500 containment intervals:  {+/- 0.0126} seconds
D: 0.9973 containment intervals:  {+/- 0.0244} seconds

R time: [04:04:56.1204]
R: 0.6800 containment intervals:  {+/- 0.0056} seconds
R: 0.9500 containment intervals:  {+/- 0.0126} seconds
R: 0.9973 containment intervals:  {+/- 0.0244} seconds

Duration (R - D): 0.1894 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0078} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0168} seconds
Duration: 0.9973 containment intervals:  {+/- 0.0299} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 20.0

fit metrics === time error bar: +/- 0.0126 seconds

fit metrics === DNR: 6.01  
fit metrics === B: 6533.15  A: 372.75 sigmaB: 1024.55  sigmaA: 527.66
fit metrics === magDrop report: percentDrop: 94.3  magDrop: 3.109  +/- 1.590  (0.95 ci)

fit metrics === D frame number: 368.0000

fit metrics === R frame number: 372.7363

fit metrics === duration: 0.1894 seconds

fit metrics === D time: [04:04:55.9310]

fit metrics === R time: [04:04:56.1204]




Data trimmed/selected using points: [103, 646]



#################### Session ended: Fri Oct  3 17:04:43 2025  ####################

