#IOTA-ES ASTEROIDAL OCCULTATION - REPORT FORM 2.01
#Event 
#Occultation: POSITIVE
#DATE: 01 October 2025
#PREDICTTIME: 20:59:22 UT
#STAR: TYC 1710-00144-1
#ASTEROID: Lintott    
#Nr: 4937
#OBSERVER
#Observer1: Jonas Schenker
#Observer2: Josef Kaeser
#moreObs:
#E-mail: j.kaeser55@bluewin.ch
#Address: CH-5015 Erlinsbach
#Observatory: Observatory Schafmatt (MPC Obs. Code: B77)
#NearestCity: Aarau
#Countrycode: CH
#Coordinates  
#Latitude: +47 25 12.9
#Longitude: +007 57 3.0
#Altitude: 820
#Datum _blank=WGS84 N=NAD1927 E=ED1950 T=Tokyo G=GB1936 *=unspecified, or other
#Datum:
#Teleskop _=unstated 1=Refractor 2=Newtonian 3=SCT 4=Dobsonian 5=Binoculars 6=Other 7=None 8=eVscope 
#Telescope: 6
#Aperture: 45
#FocalLength: 150 
#ObservingMethod   _=unspecified a=Analogue & digital video b=Digital SLR-camera video c=Photometer d=Sequential images e=Drift scan f=Visual g=Other 
#ObservingMethod: a 		    
#Observation
#StartObs:20:59:05.048
#D D=Main Star d=second Star G=satellite main star g=satellite 2nd star N=ring C=Not Seen  M=non detection +time hh:mm:ss.s
#D: D20:59:22.684
#Acc_D: 0.010
#R R=Main Star r=second Star B=satellite main star b=satellite 2nd star N=ring C=Not Seen M=non detection +time hh:mm:ss.s
#R: R020:59:23.214
#Acc_R: 0.01
#EndObs:20:59:35.120
#Duration: 0.53
#Exp_Time: 0.020
#Timesource  _=unspecified a=GPS b=NTP c=Telephone (fixed or mobile) d=Radio time signal e=Internal clock of recorder f=Stopwatch g=Other
#Timesource: a	 
#Camera: DVTI+CAM 430 
#Signal/Noise: 16.3
#Weatherconditions
#Wind: 
#Temperature:
#Transparency 1=Clear 2=Fog 3=Thin cloud <2 [mag loss <2 mag.] 4=Thick cloud >2 [mag loss >2 mag. 5=Broken opaque cloud [that is, observed thru gaps in the cloud] 6=Star faint 7=By averted vision
#Transparency: 1
#Stability _=unstated 1=Steady 2=Slight flickering 3=Strong flickering 
#Stability: 1
#Comments:
#
#EXTRA_FIELDS
#TelescopeType: Cassegrain 450 mm / f3
#MountModel: equatorial mount Baur D100
#MountMotorDrive: yes
#StartObsAccSec: 0.001
#EndObsAccSec: 0.001
#FieldOfView: 
#CameraGainDb: 24
#CameraBinning: no
#CameraWidthHeight: 1624x1240 4.5um
#CameraRecordingFormat: ADV 16-bit
#ImageSensor: Sony IMX430LLJ-C (1.1" 1624x1240 4.5um CIS)
#TimeSource: Max M8C GNSS module in the camera
#TimeInserter: -
#FrameGrabber: -
#RecordingSoftware: DVTI Cam Control V5.8.0-45
#LightcurveExtractionSoftware: Tangra v3.8.0
#LightcurveAnalysisSoftware: AOTA 4.2025.6.22
#ExtraComments:


