#IOTA-ES ASTEROIDAL OCCULTATION - REPORT FORM 2.03 - DVTI+CAM TEMPLATE 1.6
#Event
#Occultation: POSITIVE
#DATE: 03 Nov 2025, 19:09:17
#PREDICTTIME: 03 Nov 2025, 19:09:17
#STAR: TYC 4065-00053-1    
#ASTEROID: 2001 YP113  
#Nr: 99384
#OBSERVER
#Observer1: Mike Kohl
#Observer2:
#moreObs:
#E-mail: mike.kohl@gmx.ch
#Address: Tannaegertenstrasse 12, 8635 Duernten, Switzerland
#OBSERVING_STATION
#NearestCity: Reichenburg
#Countrycode: CH
#Coordinates LAT +/-DD MM SS.S  LON +/-DDD MM SS.S 
#Latitude:  +47 10 43.320
#Longitude: +008 58 15.240
#Altitude: 409
#Datum _blank=WGS84 N=NAD1927 E=ED1950 T=Tokyo G=GB1936 *=unspecified, or other
#Datum:
#Teleskop _=unstated 1=Refractor 2=Newtonian 3=SCT 4=Dobsonian 5=Binoculars 6=Other 7=None 8=eVscope 
#Telescope: 3
#Aperture in cm
#Aperture: 20.0
#FocalLength in cm
#FocalLength: 120.0 
#ObservingMethod   _=unspecified a=Analogue & digital video b=Digital SLR-camera video c=Photometer d=Sequential images e=Drift scan f=Visual g=Other 
#ObservingMethod: a 		    
#Observation
#StartObs: 19:08:39.012
#D D=Main Star d=second Star G=satellite main star g=satellite 2nd star N=ring  M=non detection +time hh:mm:ss.s
#D: D19:09:17.569
#Acc_D: 0.010
#R R=Main Star r=second Star B=satellite main star b=satellite 2nd star N=ring  M=non detection +time hh:mm:ss.s
#R: R19:09:17.809
#Acc_R: 0.010
#EndObs: 19:09:50.226
#Duration: 0.240
#Exp_Time: 0.020
#Timesource  _=unspecified a=GPS b=NTP c=Telephone (fixed or mobile) d=Radio time signal e=Internal clock of recorder f=Stopwatch g=Other
#Timesource: a	 
#Camera: DVTI+CAM 174, serial #28
#Signal/Noise: 50.2
#Weatherconditions
#Wind: 0.0
#Temperature: 5.0
#Transparency 1=Clear 2=Fog 3=Thin cloud <2 [mag loss <2 mag.] 4=Thick cloud >2 [mag loss >2 mag. 5=Broken opaque cloud [that is, observed thru gaps in the cloud] 6=Star faint 7=By averted vision
#Transparency: 3
#Stability _=unstated 1=Steady 2=Slight flickering 3=Strong flickering 
#Stability: 2
#Comments: 
#
#EXTRA_FIELDS
#Feed: Planned Observations
#MpcObsCode: -
#Prediction: no
#ProbabilityPercent: 0.0
#PredictedDurationSec: 0.5
#DistanceCentralLineKm: 15.2
#PathWidthKm: 
#StarMag:  9.3
#StarAltDeg: 41
#StarAzDeg: 39
#StarConstellation: Camelopardalis
#AsteroidMag: 17.9
#AsteroidDiameterKm:  4.0
#CombinedMag:  9.3
#DeltaMag:  8.6
#Moon: 95 percent lit, distance 65 deg
#TelescopeType: SCT
#MountModel: 
#MountMotorDrive: 
#StartObsAccSec: 0.001
#EndObsAccSec: 0.001
#FieldOfView:
#CameraGainDb: +26 dB D
#CameraBinning: 4x4
#CameraWidthHeight: 480x300
#CameraRecordingFormat: ADV 16-bit
#ImageSensor: Sony IMX174LLJ-C (1/1.2" 1920x1200 5.86um CIS)
#TimeSource: Max M8C GNSS module in the camera
#TimeInserter: -
#FrameGrabber: -
#RecordingSoftware: DVTI Cam Control v5.8.0-45
#LightcurveExtractionSoftware: 
#LightcurveAnalysisSoftware:
#ErrorInTime:  +/- 0.136 s
#StarMagnitudeInV: 
#StarMagnitudeInR: 
#MaxDuration: 0.5 s
#MagnitudeDrop:  8.6
#MagnitudeDropInR: 
#EventRank: 
#Probability: 0.0




                   ASTEROIDAL OCCULTATION - REPORT FORM

    +------------------------------+  +-------------------------------+
    |            EAON              |  |            IOTA/ES            |
    |                              |  |   INTERNATIONAL OCCULTATION   |
    |     EUROPEAN  ASTEROIDAL     |  |      TIMING  ASSOCIATION      |
    |     OCCULTATION NETWORK      |  |       EUROPEAN SECTION        |
    +------------------------------+  +-------------------------------+

1 DATE:                  2025 Nov 03, 19:09 (UTC)

  STAR:                  TYC 4065-00053-1      mv:  9.3 mag
  ASTEROID:              (99384) 2001 YP113    mv: 17.9 mag  (diam.  4.0 km)
                         combined magnitude:   mv:  9.3 mag
                         delta-magnitude:      mv:  8.6 mag

2 OBSERVER:
  Name:                  Mike Kohl
  E-mail:                mike.kohl@gmx.ch
  Address:               Tannaegertenstrasse 12, 8635 Duernten, Switzerland

3 OBSERVING STATION:
  Nearest city:          Reichenburg, CH
  Station:               RBG
  Latitude:              N47 10' 43.320" (WGS84)
  Longitude:             E008 58' 15.240" (WGS84)
  Altitude:              409 m (MSL)  (WGS84)
  Single station:        yes

  Predicted observation: no (Distance 15.2 km from C.L.)
                         Probability: 0.0 percent

                         +----------------------------------+
4 TIMING OF EVENT:       |                                  |
                         |  OCCULTATION RECORDED: POSITIVE  |
                         |                                  |
                         +----------------------------------+
  Type of event:
   S = Start observation I = Interrupt-start   D = Disappearance
   B = Blink             F = Flash             E = End observation
   I = Interrupt-end     R = Reappearance
   M = Mid-event         P = Predicted time

  Event  Time (UTC)      Acc.         Comments
  Code   HH MM SS.sss    S.sss

   S     19 08 39.012    +/-  0.001 s  : Start observation (UTC)
   E     19 09 50.226    +/-  0.001 s  : End observation   (UTC)
   P     19 09 17.418    +/-  0.136 s  : Predicted time    (UTC)
                                         (predicted: max. 0.5 s)
  
  In case of a positive event: see extracted times in the PyOTE report "LC.pyote_log.txt".
 

5 TELESCOPE: 
  Type:                  SCT
  Aperture:              200 mm
  Focal length:          1200 mm
  Magnification:         focal
  Mount:                 
  Motor drive:           

6 TIMING & RECORDING:
  Time source:           GPS
  Quality of signal:     Accuracy 1 m
  Camera/Sensor:         Digital Camera with integrated GPS-VTI (DVTI+CAM, serial #28)
                         Image Sensor Sony IMX174LLJ-C (1/1.2" 1920x1200 5.86um CIS)
                         Website of the project: https://groups.io/g/d-vti-cam/
  Settings:              480x300, Exposure time 20.0 ms, Gain +26 dB D, Binning 4x4, Format ADV 16-bit
  Time insertion:        Digital GNSS timestamp into image sensor data stream

7 OBSERVING CONDITIONS:
  Moon:                  95 percent lit, distance 65 deg
  Wind:                  0.0 Bft
  Temperature:           5.0 deg C
  Transparency:          3
  Star image stability:  2
  Altitude of star:      41 deg
  Azimut of star:        39 deg in Camelopardalis
  StarConstellation:     Camelopardalis

8 ADDITIONAL COMMENTS:
  Feed:                      Planned Observations
  Video recording software:  DVTI Cam Control v5.8.0-45
  Signal/Noise:              50.2
  Further Comments:          

