

#################### PYOTE 5.7.9  session started: Tue Nov  4 23:41:58 2025  ####################

filename: C:\Users\aschw\Desktop\20251104_4\lc.csv

==================== file header lines ====================
# PyMovie Version 4.1.5
# source: C:\Users\aschw\Desktop\DvtiData\20251104_222945_816x620_G30dBD_150.0ms.adv
#
# Aperture photometry was used to extract the lightcurves
#
# lunar background: False
# yellow mask = default: False
#
# aperture name: target
# ____ aperture size: 31
# ____ x,y: (418, 355) at frame 399
# ____ threshold: 99999
# ____ def mask radius: 2.4
# ____ color: red
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 19
#
# aperture name: tracking
# ____ aperture size: 31
# ____ x,y: (359, 366) at frame 399
# ____ threshold: 1028
# ____ def mask radius: 2.4
# ____ color: yellow
# ____ joggable: True
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 20
#
# date at frame 0: 2025-11-04
#ACQUISITION-DELAY: 0.0
#ALTITUDE: 588.7
#AUTHOR: Andreas Schweizer
#BINNING-X: 2
#BINNING-Y: 2
#CAMERA-DRIVER-NAME: UVC
#CAMERA-FIRMWARE-VERSION: 1.3.3
#CAMERA-MODEL: DVTI+CAM
#CAMERA-SENSOR-INFO: Sony IMX430LLJ-C (9.2mm 1624x1240 4.5um CIS)
#CAMERA-SERIAL-NO: 109
#CAMERA-VENDOR-NAME: DVTI
#COMMENT: 
#DEC: 58.451406
#HEIGHT: 620
#INSTRUMENT: DVTI+CAM #109 FW 1.3.3, Sensor IMX430
#LATITUDE: 47.3418449
#LONGITUDE: 8.4728732
#OBJNAME: (271666) 2004 RC55 occ. UCAC4 743-035059
#OBSERVER: Andreas Schweizer
#RA: 4.389065
#RECORDER-SOFTWARE: DvtiCamControl
#RECORDER-SOFTWARE-VERSION: 5.9.0-81
#TELESCOPE: Boren Simon
#WIDTH: 816
#
# Aperture photometry was used to extract the lightcurves
==================== end header lines ====================

No time step irregularities found.

timeDelta: 0.149997 seconds per reading
timestamp error rate: 0.00%

Home directory: C:\Users\aschw\AppData\Local\Packages\PythonSoftwareFoundation.Python.3.10_qbz5n2kfra8p0\LocalCache\local-packages\Python310\site-packages\pyoteapp

We found C:\Users\aschw\Documents\model-examples already present. Adding any new examples ...
Use min/max event to locate a "D and R" event has been selected

minEvent: 2  maxEvent: 2

Number of candidate solutions: 396 (using event min/max entries)

New solver results...

Integer (non-subframe) solution...
B:8943.68  A:1104.50
in entryNum units: D: 197  R: 199

noise corr coefs: [1.00]  (based on 397 points)  sigmaB: 1941.02

noise corr coefs: [1.00]  (based on 397 points)  sigmaB: 1941.02

Subframe adjusted solution...
B:8943.68  A:1104.50
in entryNum units: D: 197  R: 199  D(subframe): 197.0000  R(subframe): 199.0000

in frameNum units: D: 198  R: 200  D(subframe): 198.0000  R(subframe): 200.0000

... end New solver results

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1826
hiDbar   @ .68 ci:   0.1855
loDbar   @ .95 ci:  -0.4769
hiDbar   @ .95 ci:   0.4060
loDbar   @ .9973 ci:  -0.9282
hiDbar   @ .9973 ci:   0.8633

loDurBar @ .68 ci:  -0.2718
hiDurBar @ .68 ci:   0.2835
loDurBar @ .95 ci:  -0.6056
hiDurBar @ .95 ci:   0.6459
loDurBar @ .9973 ci:  -1.1055
hiDurBar @ .9973 ci:   1.1296

Timestamp validity check ...

From timestamps at D and R, calculated 2 reading blocks.  From reading blocks, calculated 2 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 8943.68  {+/- 97.54}  sigmaB: 1941.02

A: 1104.50  {+/- 807.50}  sigmaA: 807.50

magDrop report: percentDrop: 87.7  magDrop: 2.271  +/- 0.794  (0.68 ci)

DNR: 4.04

D: 198.00 {+0.19,-0.18} (frame number)
D: [22:30:15.5410]  {+0.0278,-0.0274} seconds

R: 200.00 {+0.18,-0.19} (frame number)
R: [22:30:15.8410]  {+0.0274,-0.0278} seconds

Duration (R - D): 2.0000 {+0.2776,-0.2776} readings
Duration (R - D): 0.3000 {+0.0416,-0.0416} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 8943.68  {+/- 195.08}  sigmaB: 1941.02

A: 1104.50  {+/- 1615.00}  sigmaA: 807.50

magDrop report: percentDrop: 87.7  magDrop: 2.271  +/- 1.588  (0.95 ci)

DNR: 4.04

D: 198.00 {+0.41,-0.48} (frame number)
D: [22:30:15.5410]  {+0.0609,-0.0715} seconds

R: 200.00 {+0.48,-0.41} (frame number)
R: [22:30:15.8410]  {+0.0715,-0.0609} seconds

Duration (R - D): 2.0000 {+0.6257,-0.6257} readings
Duration (R - D): 0.3000 {+0.0939,-0.0939} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 8943.68  {+/- 292.62}  sigmaB: 1941.02

A: 1104.50  {+/- 2422.50}  sigmaA: 807.50

magDrop report: percentDrop: 87.7  magDrop: 2.271  too much noise; cannot calculate error bars

DNR: 4.04

D: 198.00 {+0.86,-0.93} (frame number)
D: [22:30:15.5410]  {+0.1295,-0.1392} seconds

R: 200.00 {+0.93,-0.86} (frame number)
R: [22:30:15.8410]  {+0.1392,-0.1295} seconds

Duration (R - D): 2.0000 {+1.1176,-1.1176} readings
Duration (R - D): 0.3000 {+0.1676,-0.1676} seconds

=============== end 0.9973 containment interval report =============

D frame number: 198.00
D: 0.6800 containment intervals:  {+/- 0.19} (readings)
D: 0.9500 containment intervals:  {+/- 0.48} (readings)
D: 0.9973 containment intervals:  {+/- 0.93} (readings)

R frame number: 200.00
R: 0.6800 containment intervals:  {+/- 0.19} (readings)
R: 0.9500 containment intervals:  {+/- 0.48} (readings)
R: 0.9973 containment intervals:  {+/- 0.93} (readings)

Duration (R - D): 2.0000 readings
Duration: 0.6800 containment intervals:  {+/- 0.2776} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.6257} (readings)
Duration: 0.9973 containment intervals:  {+/- 1.1176} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.


The observed drop has a less than 3 sigma probability level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 87.7  magDrop: 2.271  +/- 1.588  (0.95 ci)

DNR: 4.04

D time: [22:30:15.5410]
D: 0.6800 containment intervals:  {+/- 0.0278} seconds
D: 0.9500 containment intervals:  {+/- 0.0715} seconds
D: 0.9973 containment intervals:  {+/- 0.1392} seconds

R time: [22:30:15.8410]
R: 0.6800 containment intervals:  {+/- 0.0278} seconds
R: 0.9500 containment intervals:  {+/- 0.0715} seconds
R: 0.9973 containment intervals:  {+/- 0.1392} seconds

Duration (R - D): 0.3000 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0416} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0939} seconds
Duration: 0.9973 containment intervals:  {+/- 0.1676} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 6.5

fit metrics === time error bar: +/- 0.0715 seconds

fit metrics === DNR: 4.04  
fit metrics === B: 8943.68  A: 1104.50 sigmaB: 1941.02  sigmaA: 807.50
fit metrics === magDrop report: percentDrop: 87.7  magDrop: 2.271  +/- 1.588  (0.95 ci)

fit metrics === D frame number: 198.0000

fit metrics === R frame number: 200.0000

fit metrics === duration: 0.3000 seconds

fit metrics === D time: [22:30:15.5410]

fit metrics === R time: [22:30:15.8410]




All data points were selected

Data trimmed/selected using points: [119, 265]

Data trimmed/selected using points: [100, 285]

