

#################### PYOTE 5.7.11  session started: Fri Nov 14 18:52:37 2025  ####################

filename: /home/nas/carsten/Polaris/Pictures/DVTI/Report/20251114_(38484) 1999 TX100/pyMovie.csv

==================== file header lines ====================
# PyMovie Version 4.1.5
# source: /home/nas/carsten/Polaris/Pictures/DVTI/Report/20251114_(38484) 1999 TX100/20251114_173907_408x310_G24dB_0060ms/20251114_173907_408x310_G24dB_0060ms.adv
#
# Aperture photometry was used to extract the lightcurves
#
# lunar background: False
# yellow mask = default: False
#
# aperture name: target
# ____ aperture size: 31
# ____ x,y: (181, 83) at frame 0
# ____ threshold: 99999
# ____ def mask radius: 2.4
# ____ color: red
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 5
#
# aperture name: track
# ____ aperture size: 31
# ____ x,y: (209, 182) at frame 0
# ____ threshold: 99999
# ____ def mask radius: 2.4
# ____ color: yellow
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 6
#
# aperture name: empty
# ____ aperture size: 31
# ____ x,y: (184, 129) at frame 0
# ____ threshold: 99999
# ____ def mask radius: 2.4
# ____ color: green
# ____ joggable: True
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 7
#
# date at frame 0: 2025-11-14
#ACQUISITION-DELAY: 0.0
#ALTITUDE: 963.6
#AUTHOR: Carsten Ziolek
#BINNING-X: 4
#BINNING-Y: 4
#CAMERA-DRIVER-NAME: UVC
#CAMERA-FIRMWARE-VERSION: 1.3.2
#CAMERA-MODEL: DVTI+CAM
#CAMERA-SENSOR-INFO: Sony IMX430LLJ-C (9.2mm 1624x1240 4.5um CIS)
#CAMERA-SERIAL-NO: 43
#CAMERA-VENDOR-NAME: DVTI
#COMMENT: 
#DEC: 15.893894
#HEIGHT: 310
#INSTRUMENT: DVTI+CAM #43 FW 1.3.2, Sensor IMX430
#LATITUDE: 46.9923429
#LONGITUDE: 9.6400521
#OBJNAME: (38484) 1999 TX100 occ. UCAC4 530-004950
#OBSERVER: Carsten Ziolek
#RA: 2.845363
#RECORDER-SOFTWARE: DvtiCamControl
#RECORDER-SOFTWARE-VERSION: 5.9.0-81
#TELESCOPE: C-14 EHD + 0.4x Red.
#WIDTH: 408
#
# Aperture photometry was used to extract the lightcurves
==================== end header lines ====================

No time step irregularities found.

timeDelta: 0.0634180 seconds per reading
timestamp error rate: 0.00%

Home directory: /home/carsten/.local/python-venv/lib/python3.10/site-packages/pyoteapp

We found /home/carsten/Documents/model-examples already present. Adding any new examples ...
signal-track is selected as the reference curve for normalization.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

Background region selected: [0, 327]

Background region selected: [584, 945]

signal-target is the light curve undergoing "selected points" noise analysis.
...This noise analysis uses 690 points

noise corr coefs: [1.00, 0.0960]  (based on 690 points)  sigmaB: 499.13

statistics of selected points:
...mean(selected points): 2474.17
...std(selected points) : 526.342
...std(detrended points): 499.127  (Warning: this sets sigmaB for the remainder of this session)
...baseline snr: 4.96  (using detrended std)

Background regions cleared.

signal-target is the target curve.

Use min/max event to locate a "D and R" event has been selected

minEvent: 1  maxEvent: 3

Number of candidate solutions: 1885 (using event min/max entries)

New solver results...

Integer (non-subframe) solution...
B:2480.89  A:622.72
in entryNum units: D: 468  R: 470

noise corr coefs: [1.00, 0.0960]  (based on 690 points)  sigmaB: 523.18

noise corr coefs: [1.00, 0.0960]  (based on 690 points)  sigmaB: 523.18

Subframe adjusted solution...
B:2480.89  A:622.72
in entryNum units: D: 468  R: 470  D(subframe): 468.0000  R(subframe): 470.0000

in frameNum units: D: 468  R: 470  D(subframe): 468.0000  R(subframe): 470.0000

... end New solver results

signal-target is the target curve.

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1566
hiDbar   @ .68 ci:   0.1694
loDbar   @ .95 ci:  -0.4408
hiDbar   @ .95 ci:   0.3632
loDbar   @ .9973 ci:  -0.8739
hiDbar   @ .9973 ci:   0.7048

loDurBar @ .68 ci:  -0.2559
hiDurBar @ .68 ci:   0.2428
loDurBar @ .95 ci:  -0.5621
hiDurBar @ .95 ci:   0.5691
loDurBar @ .9973 ci:  -1.0249
hiDurBar @ .9973 ci:   1.0292

Timestamp validity check ...

From timestamps at D and R, calculated 2 reading blocks.  From reading blocks, calculated 2 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 2480.89  {+/- 17.04}  sigmaB: 523.18

A: 622.72  {+/- 104.80}  sigmaA: 104.80

magDrop report: percentDrop: 74.9  magDrop: 1.501  +/- 0.183  (0.68 ci)

DNR: 3.55

D: 468.00 {+0.17,-0.16} (frame number)
D: [17:39:37.2020]  {+0.0107,-0.0099} seconds

R: 470.00 {+0.16,-0.17} (frame number)
R: [17:39:37.3290]  {+0.0099,-0.0107} seconds

Duration (R - D): 2.0000 {+0.2493,-0.2493} readings
Duration (R - D): 0.1270 {+0.0158,-0.0158} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 2480.89  {+/- 34.07}  sigmaB: 523.18

A: 622.72  {+/- 209.60}  sigmaA: 104.80

magDrop report: percentDrop: 74.9  magDrop: 1.501  +/- 0.366  (0.95 ci)

DNR: 3.55

D: 468.00 {+0.36,-0.44} (frame number)
D: [17:39:37.2020]  {+0.0230,-0.0280} seconds

R: 470.00 {+0.44,-0.36} (frame number)
R: [17:39:37.3290]  {+0.0280,-0.0230} seconds

Duration (R - D): 2.0000 {+0.5656,-0.5656} readings
Duration (R - D): 0.1270 {+0.0359,-0.0359} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 2480.89  {+/- 51.11}  sigmaB: 523.18

A: 622.72  {+/- 314.40}  sigmaA: 104.80

magDrop report: percentDrop: 74.9  magDrop: 1.501  +/- 0.549  (0.9973 ci)

DNR: 3.55

D: 468.00 {+0.70,-0.87} (frame number)
D: [17:39:37.2020]  {+0.0447,-0.0554} seconds

R: 470.00 {+0.87,-0.70} (frame number)
R: [17:39:37.3290]  {+0.0554,-0.0447} seconds

Duration (R - D): 2.0000 {+1.0270,-1.0270} readings
Duration (R - D): 0.1270 {+0.0651,-0.0651} seconds

=============== end 0.9973 containment interval report =============

D frame number: 468.00
D: 0.6800 containment intervals:  {+/- 0.17} (readings)
D: 0.9500 containment intervals:  {+/- 0.44} (readings)
D: 0.9973 containment intervals:  {+/- 0.87} (readings)

R frame number: 470.00
R: 0.6800 containment intervals:  {+/- 0.17} (readings)
R: 0.9500 containment intervals:  {+/- 0.44} (readings)
R: 0.9973 containment intervals:  {+/- 0.87} (readings)

Duration (R - D): 2.0000 readings
Duration: 0.6800 containment intervals:  {+/- 0.2493} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.5656} (readings)
Duration: 0.9973 containment intervals:  {+/- 1.0270} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.

This light curve has been normalized against a reference star.
... signal-track was used for normalization with X offset: 0
... 90 readings were used for smoothing



The observed drop has a less than 3 sigma probability level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 74.9  magDrop: 1.501  +/- 0.366  (0.95 ci)

DNR: 3.55

D time: [17:39:37.2020]
D: 0.6800 containment intervals:  {+/- 0.0107} seconds
D: 0.9500 containment intervals:  {+/- 0.0280} seconds
D: 0.9973 containment intervals:  {+/- 0.0554} seconds

R time: [17:39:37.3290]
R: 0.6800 containment intervals:  {+/- 0.0107} seconds
R: 0.9500 containment intervals:  {+/- 0.0280} seconds
R: 0.9973 containment intervals:  {+/- 0.0554} seconds

Duration (R - D): 0.1270 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0158} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0359} seconds
Duration: 0.9973 containment intervals:  {+/- 0.0651} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 8.4

fit metrics === time error bar: +/- 0.0280 seconds

fit metrics === DNR: 3.55  
fit metrics === B: 2480.89  A: 622.72 sigmaB: 523.18  sigmaA: 104.80
fit metrics === magDrop report: percentDrop: 74.9  magDrop: 1.501  +/- 0.366  (0.95 ci)

fit metrics === D frame number: 468.0000

fit metrics === R frame number: 470.0000

fit metrics === duration: 0.1270 seconds

fit metrics === D time: [17:39:37.2020]

fit metrics === R time: [17:39:37.3290]




signal-target is the target curve.

Data trimmed/selected using points: [417, 514]

signal-target is the target curve.

signal-target is the target curve.



#################### Session ended: Fri Nov 14 18:59:41 2025  ####################

