

#################### PYOTE 5.7.11  session started: Tue Feb  3 20:00:57 2026  ####################

filename: /home/nas/carsten/Polaris/Pictures/DVTI/Report/20260203_(201161) 2002 LF35/pyMovie.csv

==================== file header lines ====================
# PyMovie Version 4.1.5
# source: /home/nas/carsten/Polaris/Pictures/DVTI/Report/20260203_(201161) 2002 LF35/20260203_184446_816x620_G24dB_0080ms/20260203_184446_816x620_G24dB_0080ms.adv
#
# Aperture photometry was used to extract the lightcurves
#
# lunar background: False
# yellow mask = default: False
#
# aperture name: target
# ____ aperture size: 31
# ____ x,y: (412, 288) at frame 749
# ____ threshold: 99999
# ____ def mask radius: 2.0
# ____ color: red
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 0
#
# aperture name: track
# ____ aperture size: 31
# ____ x,y: (417, 386) at frame 749
# ____ threshold: 99999
# ____ def mask radius: 2.0
# ____ color: yellow
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 1
#
# aperture name: empty
# ____ aperture size: 31
# ____ x,y: (414, 336) at frame 749
# ____ threshold: 99999
# ____ def mask radius: 2.0
# ____ color: green
# ____ joggable: True
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 2
#
# date at frame 0: 2026-02-03
#ACQUISITION-DELAY: 0.0
#ALTITUDE: 922.6
#AUTHOR: Carsten Ziolek
#BINNING-X: 2
#BINNING-Y: 2
#CAMERA-DRIVER-NAME: UVC
#CAMERA-FIRMWARE-VERSION: 1.3.2
#CAMERA-MODEL: DVTI+CAM
#CAMERA-SENSOR-INFO: Sony IMX430LLJ-C (9.2mm 1624x1240 4.5um CIS)
#CAMERA-SERIAL-NO: 43
#CAMERA-VENDOR-NAME: DVTI
#COMMENT: 
#DEC: 42.366011
#HEIGHT: 620
#INSTRUMENT: DVTI+CAM #43 FW 1.3.2, Sensor IMX430
#LATITUDE: 46.9925389
#LONGITUDE: 9.6397842
#OBJNAME: (201161) 2002 LF35 occ. UCAC4 662-012704
#OBSERVER: Carsten Ziolek
#RA: 2.869027
#RECORDER-SOFTWARE: DvtiCamControl
#RECORDER-SOFTWARE-VERSION: 5.9.0-81
#TELESCOPE: C-14 EHD + 0.4x Red.
#WIDTH: 816
#
# Aperture photometry was used to extract the lightcurves
==================== end header lines ====================

No time step irregularities found.

timeDelta: 0.0799960 seconds per reading
timestamp error rate: 0.00%

Home directory: /home/carsten/.local/python-venv/lib/python3.10/site-packages/pyoteapp

We found /home/carsten/Documents/model-examples already present. Adding any new examples ...
signal-track is selected as the reference curve for normalization.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

signal-target is the target curve.

Use min/max event to locate a "D and R" event has been selected

minEvent: 5  maxEvent: 10

Number of candidate solutions: 4449 (using event min/max entries)

New solver results...

Integer (non-subframe) solution...
B:2972.12  A:447.62
in entryNum units: D: 373  R: 380

noise corr coefs: [1.00, 0.0506, 0.0693]  (based on 743 points)  sigmaB: 596.89

noise corr coefs: [1.00, 0.0506, 0.0693]  (based on 743 points)  sigmaB: 596.89

Subframe adjusted solution...
B:2972.12  A:447.62
in entryNum units: D: 373  R: 380  D(subframe): 373.0000  R(subframe): 380.0000

in frameNum units: D: 373  R: 380  D(subframe): 373.0000  R(subframe): 380.0000

... end New solver results

signal-target is the target curve.

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1969
hiDbar   @ .68 ci:   0.1985
loDbar   @ .95 ci:  -0.5080
hiDbar   @ .95 ci:   0.4415
loDbar   @ .9973 ci:  -0.9908
hiDbar   @ .9973 ci:   0.8902

loDurBar @ .68 ci:  -0.2988
hiDurBar @ .68 ci:   0.2950
loDurBar @ .95 ci:  -0.6855
hiDurBar @ .95 ci:   0.6463
loDurBar @ .9973 ci:  -1.2003
hiDurBar @ .9973 ci:   1.1793

Timestamp validity check ...

From timestamps at D and R, calculated 7 reading blocks.  From reading blocks, calculated 7 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 2972.12  {+/- 21.91}  sigmaB: 596.89

A: 447.62  {+/- 131.60}  sigmaA: 322.36

magDrop report: percentDrop: 84.9  magDrop: 2.055  +/- 0.319  (0.68 ci)

DNR: 4.23

D: 373.00 {+0.20,-0.20} (frame number)
D: [18:45:16.2790]  {+0.0159,-0.0157} seconds

R: 380.00 {+0.20,-0.20} (frame number)
R: [18:45:16.8390]  {+0.0157,-0.0159} seconds

Duration (R - D): 7.0000 {+0.2969,-0.2969} readings
Duration (R - D): 0.5600 {+0.0237,-0.0237} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 2972.12  {+/- 43.83}  sigmaB: 596.89

A: 447.62  {+/- 263.21}  sigmaA: 322.36

magDrop report: percentDrop: 84.9  magDrop: 2.055  +/- 0.639  (0.95 ci)

DNR: 4.23

D: 373.00 {+0.44,-0.51} (frame number)
D: [18:45:16.2790]  {+0.0353,-0.0406} seconds

R: 380.00 {+0.51,-0.44} (frame number)
R: [18:45:16.8390]  {+0.0406,-0.0353} seconds

Duration (R - D): 7.0000 {+0.6659,-0.6659} readings
Duration (R - D): 0.5600 {+0.0533,-0.0533} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 2972.12  {+/- 65.74}  sigmaB: 596.89

A: 447.62  {+/- 394.81}  sigmaA: 322.36

magDrop report: percentDrop: 84.9  magDrop: 2.055  +/- 0.958  (0.9973 ci)

DNR: 4.23

D: 373.00 {+0.89,-0.99} (frame number)
D: [18:45:16.2790]  {+0.0712,-0.0793} seconds

R: 380.00 {+0.99,-0.89} (frame number)
R: [18:45:16.8390]  {+0.0793,-0.0712} seconds

Duration (R - D): 7.0000 {+1.1898,-1.1898} readings
Duration (R - D): 0.5600 {+0.0952,-0.0952} seconds

=============== end 0.9973 containment interval report =============

D frame number: 373.00
D: 0.6800 containment intervals:  {+/- 0.20} (readings)
D: 0.9500 containment intervals:  {+/- 0.51} (readings)
D: 0.9973 containment intervals:  {+/- 0.99} (readings)

R frame number: 380.00
R: 0.6800 containment intervals:  {+/- 0.20} (readings)
R: 0.9500 containment intervals:  {+/- 0.51} (readings)
R: 0.9973 containment intervals:  {+/- 0.99} (readings)

Duration (R - D): 7.0000 readings
Duration: 0.6800 containment intervals:  {+/- 0.2969} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.6659} (readings)
Duration: 0.9973 containment intervals:  {+/- 1.1898} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.

This light curve has been normalized against a reference star.
... signal-track was used for normalization with X offset: 0
... 44 readings were used for smoothing



The observed drop has an estimated 9.6 sigma level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 84.9  magDrop: 2.055  +/- 0.639  (0.95 ci)

DNR: 4.23

D time: [18:45:16.2790]
D: 0.6800 containment intervals:  {+/- 0.0159} seconds
D: 0.9500 containment intervals:  {+/- 0.0406} seconds
D: 0.9973 containment intervals:  {+/- 0.0793} seconds

R time: [18:45:16.8390]
R: 0.6800 containment intervals:  {+/- 0.0159} seconds
R: 0.9500 containment intervals:  {+/- 0.0406} seconds
R: 0.9973 containment intervals:  {+/- 0.0793} seconds

Duration (R - D): 0.5600 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0237} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0533} seconds
Duration: 0.9973 containment intervals:  {+/- 0.0952} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 14.7

fit metrics === time error bar: +/- 0.0406 seconds

fit metrics === DNR: 4.23  
fit metrics === B: 2972.12  A: 447.62 sigmaB: 596.89  sigmaA: 322.36
fit metrics === magDrop report: percentDrop: 84.9  magDrop: 2.055  +/- 0.639  (0.95 ci)

fit metrics === D frame number: 373.0000

fit metrics === R frame number: 380.0000

fit metrics === duration: 0.5600 seconds

fit metrics === D time: [18:45:16.2790]

fit metrics === R time: [18:45:16.8390]




signal-target is the target curve.

Data trimmed/selected using points: [255, 496]

signal-target is the target curve.

signal-target is the target curve.

Background region selected: [0, 348]

Background region selected: [391, 749]

signal-target is the light curve undergoing "selected points" noise analysis.
...This noise analysis uses 708 points

noise corr coefs: [1.00]  (based on 708 points)  sigmaB: 579.57

statistics of selected points:
...mean(selected points): 2967.72
...std(selected points) : 594.464
...std(detrended points): 579.568  (Warning: this sets sigmaB for the remainder of this session)
...baseline snr: 5.12  (using detrended std)

Background regions cleared.

signal-target is the target curve.



#################### Session ended: Tue Feb  3 20:06:56 2026  ####################

