#IOTA-ES ASTEROIDAL OCCULTATION - REPORT FORM 2.03 - DVTI+CAM TEMPLATE 1.6
#Event
#Occultation: NEGATIVE
#DATE: 03 Feb 2026, 18:19:18
#PREDICTTIME: 03 Feb 2026, 18:19:18
#STAR: UCAC4 628-019156    
#ASTEROID: 2000 GZ9       
#Nr: 76493
#OBSERVER
#Observer1: Mike Kohl
#Observer2:
#moreObs:
#E-mail: mike.kohl@gmx.ch
#Address: Tannaegertenstrasse 12, 8635 Duernten, Switzerland
#OBSERVING_STATION
#NearestCity: Duernten
#Countrycode: CH
#Coordinates LAT +/-DD MM SS.S  LON +/-DDD MM SS.S 
#Latitude:  +47 16 36.998
#Longitude: +008 50 16.598
#Altitude: 511
#Datum _blank=WGS84 N=NAD1927 E=ED1950 T=Tokyo G=GB1936 *=unspecified, or other
#Datum:
#Teleskop _=unstated 1=Refractor 2=Newtonian 3=SCT 4=Dobsonian 5=Binoculars 6=Other 7=None 8=eVscope 
#Telescope: 3
#Aperture in cm
#Aperture: 20.0
#FocalLength in cm
#FocalLength: 120.0 
#ObservingMethod   _=unspecified a=Analogue & digital video b=Digital SLR-camera video c=Photometer d=Sequential images e=Drift scan f=Visual g=Other 
#ObservingMethod: a 		    
#Observation
#StartObs: 18:18:24.56
#D D=Main Star d=second Star G=satellite main star g=satellite 2nd star N=ring  M=non detection +time hh:mm:ss.s
#D: M            
#Acc_D:      
#R R=Main Star r=second Star B=satellite main star b=satellite 2nd star N=ring  M=non detection +time hh:mm:ss.s
#R: M            
#Acc_R:      
#EndObs: 18:20:02.57
#Duration:      
#Exp_Time: 0.200
#Timesource  _=unspecified a=GPS b=NTP c=Telephone (fixed or mobile) d=Radio time signal e=Internal clock of recorder f=Stopwatch g=Other
#Timesource: a	 
#Camera: DVTI+CAM 174, serial #28
#Signal/Noise: 
#Weatherconditions
#Wind: 0.0
#Temperature: 4.0
#Transparency 1=Clear 2=Fog 3=Thin cloud <2 [mag loss <2 mag.] 4=Thick cloud >2 [mag loss >2 mag. 5=Broken opaque cloud [that is, observed thru gaps in the cloud] 6=Star faint 7=By averted vision
#Transparency: 1
#Stability _=unstated 1=Steady 2=Slight flickering 3=Strong flickering 
#Stability: 2
#Comments: 
#
#EXTRA_FIELDS
#Feed: {{EVENT_FEED_NAME}}
#MpcObsCode: -
#Prediction: no
#ProbabilityPercent: 0.0
#PredictedDurationSec: 0.5
#DistanceCentralLineKm: {{EVENT_DISTANCE_CENTRAL_LINE}}
#PathWidthKm: 
#StarMag: 12.6
#StarAltDeg: {{EVENT_STAR_ALTITUDE}}
#StarAzDeg: {{EVENT_STAR_AZIMUT}}
#StarConstellation: {{EVENT_STAR_CONSTELLATION}}
#AsteroidMag: 19.3
#AsteroidDiameterKm: {{EVENT_ASTEROID_DIAMETER}}
#CombinedMag: 11.9
#DeltaMag:  6.7
#Moon: {{EVENT_MOON_INFO}}
#TelescopeType: SCT
#MountModel: 
#MountMotorDrive: 
#StartObsAccSec: X.XXX
#EndObsAccSec: X.XXX
#FieldOfView:
#CameraGainDb: {{CAMERA_GAIN}}
#CameraBinning: {{CAMERA_BINNING}}
#CameraWidthHeight: {{CAMERA_W_H}}
#CameraRecordingFormat: {{RECORDING_FORMAT}}
#ImageSensor: {{CAMERA_SENSOR_NAME}}
#TimeSource: Max M8C GNSS module in the camera
#TimeInserter: -
#FrameGrabber: -
#RecordingSoftware: DVTI Cam Control v5.8.0-45
#LightcurveExtractionSoftware: 
#LightcurveAnalysisSoftware:
#ErrorInTime:  +/- 0.000 s
#StarMagnitudeInV: 
#StarMagnitudeInR: 
#MaxDuration: 0.5 s
#MagnitudeDrop:  6.7
#MagnitudeDropInR: 
#EventRank: 
#Probability: 0.0




                   ASTEROIDAL OCCULTATION - REPORT FORM

    +------------------------------+  +-------------------------------+
    |            EAON              |  |            IOTA/ES            |
    |                              |  |   INTERNATIONAL OCCULTATION   |
    |     EUROPEAN  ASTEROIDAL     |  |      TIMING  ASSOCIATION      |
    |     OCCULTATION NETWORK      |  |       EUROPEAN SECTION        |
    +------------------------------+  +-------------------------------+

1 DATE:                  2026 Feb 03, 18:19 (UTC)

  STAR:                  UCAC4 628-019156      mv: 12.6 mag
  ASTEROID:              76493 2000GZ9         mv: 19.3 mag  (diam. {{EVENT_ASTEROID_DIAMETER}} km)
                         combined magnitude:   mv: 11.9 mag
                         delta-magnitude:      mv:  6.7 mag

2 OBSERVER:
  Name:                  Mike Kohl
  E-mail:                mike.kohl@gmx.ch
  Address:               Tannaegertenstrasse 12, 8635 Duernten, Switzerland

3 OBSERVING STATION:
  Nearest city:          Duernten, CH
  Station:               DUE
  Latitude:              N47 16' 36.998" (WGS84)
  Longitude:             E008 50' 16.598" (WGS84)
  Altitude:              511 m (MSL)  (WGS84)
  Single station:        yes

  Predicted observation: no (Distance {{EVENT_DISTANCE_CENTRAL_LINE}} km from C.L.)
                         Probability: 0.0 percent

                         +----------------------------------+
4 TIMING OF EVENT:       |                                  |
                         |  OCCULTATION RECORDED: NEGATIVE  |
                         |                                  |
                         +----------------------------------+
  Type of event:
   S = Start observation I = Interrupt-start   D = Disappearance
   B = Blink             F = Flash             E = End observation
   I = Interrupt-end     R = Reappearance
   M = Mid-event         P = Predicted time

  Event  Time (UTC)      Acc.         Comments
  Code   HH MM SS.sss    S.sss

   S     XX XX XX.XXX    +/-  X.XXX s  : Start observation (UTC)
   E     XX XX XX.XXX    +/-  X.XXX s  : End observation   (UTC)
   P     18 19 18.000    +/-  0.000 s  : Predicted time    (UTC)
                                         (predicted: max. 0.5 s)
  
  In case of a positive event: see extracted times in the PyOTE report "LC.pyote_log.txt".
 

5 TELESCOPE: 
  Type:                  SCT
  Aperture:              200 mm
  Focal length:          1200 mm
  Magnification:         focal
  Mount:                 
  Motor drive:           

6 TIMING & RECORDING:
  Time source:           GPS
  Quality of signal:     Accuracy n/a m
  Camera/Sensor:         Digital Camera with integrated GPS-VTI ({{CAMERA_MODEL_NAME}}, serial #{{CAMERA_SERIAL_NR}})
                         Image Sensor {{CAMERA_SENSOR_NAME}}
                         Website of the project: https://groups.io/g/d-vti-cam/
  Settings:              {{CAMERA_W_H}}, Exposure time {{CAMERA_EXPOSURE_TIME}}, Gain {{CAMERA_GAIN}}, Binning {{CAMERA_BINNING}}, Format {{RECORDING_FORMAT}}
  Time insertion:        Digital GNSS timestamp into image sensor data stream

7 OBSERVING CONDITIONS:
  Moon:                  {{EVENT_MOON_INFO}}
  Wind:                  0.0 Bft
  Temperature:           4.0 deg C
  Transparency:          1
  Star image stability:  2
  Altitude of star:      {{EVENT_STAR_ALTITUDE}} deg
  Azimut of star:        {{EVENT_STAR_AZIMUT}} deg in {{EVENT_STAR_CONSTELLATION}}
  StarConstellation:     {{EVENT_STAR_CONSTELLATION}}

8 ADDITIONAL COMMENTS:
  Feed:                      {{EVENT_FEED_NAME}}
  Video recording software:  DVTI Cam Control v5.8.0-45
  Signal/Noise:              
  Further Comments:          

