

#################### PYOTE 5.7.9  session started: Wed Oct  1 22:19:29 2025  ####################

filename: C:\Users\aschw\Desktop\vj213.csv

==================== file header lines ====================
# PyMovie Version 4.1.5
# source: C:\Users\aschw\Desktop\DvtiData\20251001_200329_816x620_G30dBD_150.0ms.adv
#
# Aperture photometry was used to extract the lightcurves
#
# lunar background: False
# yellow mask = default: False
#
# aperture name: target
# ____ aperture size: 31
# ____ x,y: (397, 306) at frame 399
# ____ threshold: 886
# ____ def mask radius: 3.2
# ____ color: red
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 0
#
# aperture name: tracking
# ____ aperture size: 31
# ____ x,y: (363, 297) at frame 399
# ____ threshold: 1106
# ____ def mask radius: 3.2
# ____ color: yellow
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 1
#
# aperture name: ref
# ____ aperture size: 31
# ____ x,y: (308, 229) at frame 399
# ____ threshold: 854
# ____ def mask radius: 3.2
# ____ color: green
# ____ joggable: True
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 2
#
# date at frame 0: 2025-10-01
#ACQUISITION-DELAY: 0.0
#ALTITUDE: 573.2
#AUTHOR: Andreas Schweizer
#BINNING-X: 2
#BINNING-Y: 2
#CAMERA-DRIVER-NAME: UVC
#CAMERA-FIRMWARE-VERSION: 1.3.3
#CAMERA-MODEL: DVTI+CAM
#CAMERA-SENSOR-INFO: Sony IMX430LLJ-C (9.2mm 1624x1240 4.5um CIS)
#CAMERA-SERIAL-NO: 109
#CAMERA-VENDOR-NAME: DVTI
#COMMENT: 
#DEC: -9.439492
#HEIGHT: 620
#INSTRUMENT: DVTI+CAM #109 FW 1.3.3, Sensor IMX430
#LATITUDE: 47.3419373
#LONGITUDE: 8.4728637
#OBJNAME: (92055) 1999 VJ213 occ. UCAC4 403-126558
#OBSERVER: Andreas Schweizer
#RA: 20.000707
#RECORDER-SOFTWARE: DvtiCamControl
#RECORDER-SOFTWARE-VERSION: 5.9.0-81
#TELESCOPE: Boren Simon
#WIDTH: 816
#
# Aperture photometry was used to extract the lightcurves
==================== end header lines ====================

No time step irregularities found.

timeDelta: 0.149995 seconds per reading
timestamp error rate: 0.00%

Home directory: C:\Users\aschw\AppData\Local\Packages\PythonSoftwareFoundation.Python.3.10_qbz5n2kfra8p0\LocalCache\local-packages\Python310\site-packages\pyoteapp

We found C:\Users\aschw\Documents\model-examples already present. Adding any new examples ...
Use min/max event to locate a "D and R" event has been selected

D zone selected: [113, 194]

R zone selected: [196, 271]

Locate a "D and R" event has been selected

Number of candidate solutions: 6232 (using D/R region selections)

New solver results...

Integer (non-subframe) solution...
B:12902.93  A:123.33
in entryNum units: D: 193  R: 196

noise corr coefs: [1.00, 0.0788]  (based on 397 points)  sigmaB: 2934.73

noise corr coefs: [1.00, 0.0905]  (based on 396 points)  sigmaB: 2930.68

Subframe adjusted solution...
B:12913.63  A:123.33
in entryNum units: D: 192  R: 196  D(subframe): 192.6682  R(subframe): 196.0000

in frameNum units: D: 192  R: 196  D(subframe): 192.6682  R(subframe): 196.0000

... end New solver results

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1386
hiDbar   @ .68 ci:   0.1455
loDbar   @ .95 ci:  -0.3618
hiDbar   @ .95 ci:   0.3211
loDbar   @ .9973 ci:  -0.7122
hiDbar   @ .9973 ci:   0.6391

loDurBar @ .68 ci:  -0.2093
hiDurBar @ .68 ci:   0.2186
loDurBar @ .95 ci:  -0.4645
hiDurBar @ .95 ci:   0.5008
loDurBar @ .9973 ci:  -0.8451
hiDurBar @ .9973 ci:   0.8375

Timestamp validity check ...

From timestamps at D and R, calculated 4 reading blocks.  From reading blocks, calculated 4 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 12913.63  {+/- 147.33}  sigmaB: 2930.68

A: 123.33  {+/- 499.14}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  +/- 4.394  (0.68 ci)

DNR: 4.36

D: 192.67 {+0.15,-0.14} (frame number)
D: [20:03:58.7632]  {+0.0218,-0.0208} seconds

R: 196.00 {+0.14,-0.15} (frame number)
R: [20:03:59.2630]  {+0.0208,-0.0218} seconds

Duration (R - D): 3.3318 {+0.2140,-0.2140} readings
Duration (R - D): 0.4998 {+0.0321,-0.0321} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 12913.63  {+/- 294.67}  sigmaB: 2930.68

A: 123.33  {+/- 998.28}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D: 192.67 {+0.32,-0.36} (frame number)
D: [20:03:58.7632]  {+0.0482,-0.0543} seconds

R: 196.00 {+0.36,-0.32} (frame number)
R: [20:03:59.2630]  {+0.0543,-0.0482} seconds

Duration (R - D): 3.3318 {+0.4827,-0.4827} readings
Duration (R - D): 0.4998 {+0.0724,-0.0724} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 12913.63  {+/- 442.00}  sigmaB: 2930.68

A: 123.33  {+/- 1497.42}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D: 192.67 {+0.64,-0.71} (frame number)
D: [20:03:58.7632]  {+0.0959,-0.1068} seconds

R: 196.00 {+0.71,-0.64} (frame number)
R: [20:03:59.2630]  {+0.1068,-0.0959} seconds

Duration (R - D): 3.3318 {+0.8413,-0.8413} readings
Duration (R - D): 0.4998 {+0.1262,-0.1262} seconds

=============== end 0.9973 containment interval report =============

D frame number: 192.67
D: 0.6800 containment intervals:  {+/- 0.15} (readings)
D: 0.9500 containment intervals:  {+/- 0.36} (readings)
D: 0.9973 containment intervals:  {+/- 0.71} (readings)

R frame number: 196.00
R: 0.6800 containment intervals:  {+/- 0.15} (readings)
R: 0.9500 containment intervals:  {+/- 0.36} (readings)
R: 0.9973 containment intervals:  {+/- 0.71} (readings)

Duration (R - D): 3.3318 readings
Duration: 0.6800 containment intervals:  {+/- 0.2140} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.4827} (readings)
Duration: 0.9973 containment intervals:  {+/- 0.8413} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.


The observed drop has an estimated 6.4 sigma level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D time: [20:03:58.7632]
D: 0.6800 containment intervals:  {+/- 0.0218} seconds
D: 0.9500 containment intervals:  {+/- 0.0543} seconds
D: 0.9973 containment intervals:  {+/- 0.1068} seconds

R time: [20:03:59.2630]
R: 0.6800 containment intervals:  {+/- 0.0218} seconds
R: 0.9500 containment intervals:  {+/- 0.0543} seconds
R: 0.9973 containment intervals:  {+/- 0.1068} seconds

Duration (R - D): 0.4998 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0321} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0724} seconds
Duration: 0.9973 containment intervals:  {+/- 0.1262} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 20.7

fit metrics === time error bar: +/- 0.0543 seconds

fit metrics === DNR: 4.36  
fit metrics === B: 12913.63  A: 123.33 sigmaB: 2930.68  sigmaA: 762.20
fit metrics === magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

fit metrics === D frame number: 192.6682

fit metrics === R frame number: 196.0000

fit metrics === duration: 0.4998 seconds

fit metrics === D time: [20:03:58.7632]

fit metrics === R time: [20:03:59.2630]




Locate a "D and R" event has been selected

Number of candidate solutions: 6232 (using D/R region selections)

New solver results...

Integer (non-subframe) solution...
B:12902.93  A:123.33
in entryNum units: D: 193  R: 196

noise corr coefs: [1.00, 0.0788]  (based on 397 points)  sigmaB: 2934.73

noise corr coefs: [1.00, 0.0905]  (based on 396 points)  sigmaB: 2930.68

Subframe adjusted solution...
B:12913.63  A:123.33
in entryNum units: D: 192  R: 196  D(subframe): 192.6682  R(subframe): 196.0000

in frameNum units: D: 192  R: 196  D(subframe): 192.6682  R(subframe): 196.0000

... end New solver results

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1370
hiDbar   @ .68 ci:   0.1485
loDbar   @ .95 ci:  -0.3779
hiDbar   @ .95 ci:   0.3150
loDbar   @ .9973 ci:  -0.6876
hiDbar   @ .9973 ci:   0.6666

loDurBar @ .68 ci:  -0.2131
hiDurBar @ .68 ci:   0.2192
loDurBar @ .95 ci:  -0.4790
hiDurBar @ .95 ci:   0.4938
loDurBar @ .9973 ci:  -0.8593
hiDurBar @ .9973 ci:   0.8784

Timestamp validity check ...

From timestamps at D and R, calculated 4 reading blocks.  From reading blocks, calculated 4 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 12913.63  {+/- 147.33}  sigmaB: 2930.68

A: 123.33  {+/- 499.14}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  +/- 4.394  (0.68 ci)

DNR: 4.36

D: 192.67 {+0.15,-0.14} (frame number)
D: [20:03:58.7632]  {+0.0223,-0.0206} seconds

R: 196.00 {+0.14,-0.15} (frame number)
R: [20:03:59.2630]  {+0.0206,-0.0223} seconds

Duration (R - D): 3.3318 {+0.2162,-0.2162} readings
Duration (R - D): 0.4998 {+0.0324,-0.0324} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 12913.63  {+/- 294.67}  sigmaB: 2930.68

A: 123.33  {+/- 998.28}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D: 192.67 {+0.32,-0.38} (frame number)
D: [20:03:58.7632]  {+0.0473,-0.0567} seconds

R: 196.00 {+0.38,-0.32} (frame number)
R: [20:03:59.2630]  {+0.0567,-0.0473} seconds

Duration (R - D): 3.3318 {+0.4864,-0.4864} readings
Duration (R - D): 0.4998 {+0.0730,-0.0730} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 12913.63  {+/- 442.00}  sigmaB: 2930.68

A: 123.33  {+/- 1497.42}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D: 192.67 {+0.67,-0.69} (frame number)
D: [20:03:58.7632]  {+0.1000,-0.1031} seconds

R: 196.00 {+0.69,-0.67} (frame number)
R: [20:03:59.2630]  {+0.1031,-0.1000} seconds

Duration (R - D): 3.3318 {+0.8688,-0.8688} readings
Duration (R - D): 0.4998 {+0.1303,-0.1303} seconds

=============== end 0.9973 containment interval report =============

D frame number: 192.67
D: 0.6800 containment intervals:  {+/- 0.15} (readings)
D: 0.9500 containment intervals:  {+/- 0.38} (readings)
D: 0.9973 containment intervals:  {+/- 0.69} (readings)

R frame number: 196.00
R: 0.6800 containment intervals:  {+/- 0.15} (readings)
R: 0.9500 containment intervals:  {+/- 0.38} (readings)
R: 0.9973 containment intervals:  {+/- 0.69} (readings)

Duration (R - D): 3.3318 readings
Duration: 0.6800 containment intervals:  {+/- 0.2162} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.4864} (readings)
Duration: 0.9973 containment intervals:  {+/- 0.8688} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.


The observed drop has an estimated 6.5 sigma level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D time: [20:03:58.7632]
D: 0.6800 containment intervals:  {+/- 0.0223} seconds
D: 0.9500 containment intervals:  {+/- 0.0567} seconds
D: 0.9973 containment intervals:  {+/- 0.1031} seconds

R time: [20:03:59.2630]
R: 0.6800 containment intervals:  {+/- 0.0223} seconds
R: 0.9500 containment intervals:  {+/- 0.0567} seconds
R: 0.9973 containment intervals:  {+/- 0.1031} seconds

Duration (R - D): 0.4998 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0324} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0730} seconds
Duration: 0.9973 containment intervals:  {+/- 0.1303} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 20.2

fit metrics === time error bar: +/- 0.0567 seconds

fit metrics === DNR: 4.36  
fit metrics === B: 12913.63  A: 123.33 sigmaB: 2930.68  sigmaA: 762.20
fit metrics === magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

fit metrics === D frame number: 192.6682

fit metrics === R frame number: 196.0000

fit metrics === duration: 0.4998 seconds

fit metrics === D time: [20:03:58.7632]

fit metrics === R time: [20:03:59.2630]




All data points were selected

All data points were selected

All data points were selected

Locate a "D and R" event has been selected

Number of candidate solutions: 6232 (using D/R region selections)

New solver results...

Integer (non-subframe) solution...
B:12902.93  A:123.33
in entryNum units: D: 193  R: 196

noise corr coefs: [1.00, 0.0788]  (based on 397 points)  sigmaB: 2934.73

noise corr coefs: [1.00, 0.0905]  (based on 396 points)  sigmaB: 2930.68

Subframe adjusted solution...
B:12913.63  A:123.33
in entryNum units: D: 192  R: 196  D(subframe): 192.6682  R(subframe): 196.0000

in frameNum units: D: 192  R: 196  D(subframe): 192.6682  R(subframe): 196.0000

... end New solver results

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1352
hiDbar   @ .68 ci:   0.1511
loDbar   @ .95 ci:  -0.3757
hiDbar   @ .95 ci:   0.3106
loDbar   @ .9973 ci:  -0.7533
hiDbar   @ .9973 ci:   0.6116

loDurBar @ .68 ci:  -0.2134
hiDurBar @ .68 ci:   0.2192
loDurBar @ .95 ci:  -0.4936
hiDurBar @ .95 ci:   0.4799
loDurBar @ .9973 ci:  -0.8534
hiDurBar @ .9973 ci:   0.9038

Timestamp validity check ...

From timestamps at D and R, calculated 4 reading blocks.  From reading blocks, calculated 4 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 12913.63  {+/- 147.33}  sigmaB: 2930.68

A: 123.33  {+/- 499.14}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  +/- 4.394  (0.68 ci)

DNR: 4.36

D: 192.67 {+0.15,-0.14} (frame number)
D: [20:03:58.7632]  {+0.0227,-0.0203} seconds

R: 196.00 {+0.14,-0.15} (frame number)
R: [20:03:59.2630]  {+0.0203,-0.0227} seconds

Duration (R - D): 3.3318 {+0.2163,-0.2163} readings
Duration (R - D): 0.4998 {+0.0324,-0.0324} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 12913.63  {+/- 294.67}  sigmaB: 2930.68

A: 123.33  {+/- 998.28}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D: 192.67 {+0.31,-0.38} (frame number)
D: [20:03:58.7632]  {+0.0466,-0.0563} seconds

R: 196.00 {+0.38,-0.31} (frame number)
R: [20:03:59.2630]  {+0.0563,-0.0466} seconds

Duration (R - D): 3.3318 {+0.4868,-0.4868} readings
Duration (R - D): 0.4998 {+0.0730,-0.0730} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 12913.63  {+/- 442.00}  sigmaB: 2930.68

A: 123.33  {+/- 1497.42}  sigmaA: 762.20

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D: 192.67 {+0.61,-0.75} (frame number)
D: [20:03:58.7632]  {+0.0917,-0.1130} seconds

R: 196.00 {+0.75,-0.61} (frame number)
R: [20:03:59.2630]  {+0.1130,-0.0917} seconds

Duration (R - D): 3.3318 {+0.8786,-0.8786} readings
Duration (R - D): 0.4998 {+0.1318,-0.1318} seconds

=============== end 0.9973 containment interval report =============

D frame number: 192.67
D: 0.6800 containment intervals:  {+/- 0.15} (readings)
D: 0.9500 containment intervals:  {+/- 0.38} (readings)
D: 0.9973 containment intervals:  {+/- 0.75} (readings)

R frame number: 196.00
R: 0.6800 containment intervals:  {+/- 0.15} (readings)
R: 0.9500 containment intervals:  {+/- 0.38} (readings)
R: 0.9973 containment intervals:  {+/- 0.75} (readings)

Duration (R - D): 3.3318 readings
Duration: 0.6800 containment intervals:  {+/- 0.2163} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.4868} (readings)
Duration: 0.9973 containment intervals:  {+/- 0.8786} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.


The observed drop has an estimated 6.5 sigma level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

DNR: 4.36

D time: [20:03:58.7632]
D: 0.6800 containment intervals:  {+/- 0.0227} seconds
D: 0.9500 containment intervals:  {+/- 0.0563} seconds
D: 0.9973 containment intervals:  {+/- 0.1130} seconds

R time: [20:03:59.2630]
R: 0.6800 containment intervals:  {+/- 0.0227} seconds
R: 0.9500 containment intervals:  {+/- 0.0563} seconds
R: 0.9973 containment intervals:  {+/- 0.1130} seconds

Duration (R - D): 0.4998 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0324} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0730} seconds
Duration: 0.9973 containment intervals:  {+/- 0.1318} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 20.4

fit metrics === time error bar: +/- 0.0563 seconds

fit metrics === DNR: 4.36  
fit metrics === B: 12913.63  A: 123.33 sigmaB: 2930.68  sigmaA: 762.20
fit metrics === magDrop report: percentDrop: 99.0  magDrop: 5.050  too much noise; cannot calculate error bars

fit metrics === D frame number: 192.6682

fit metrics === R frame number: 196.0000

fit metrics === duration: 0.4998 seconds

fit metrics === D time: [20:03:58.7632]

fit metrics === R time: [20:03:59.2630]




Data trimmed/selected using points: [169, 220]

Data trimmed/selected using points: [124, 248]

Data trimmed/selected using points: [107, 272]

