

#################### PYOTE 5.7.9  session started: Tue Nov  4 20:47:43 2025  ####################

filename: C:\Users\aschw\Desktop\20251104_1\lc.csv

==================== file header lines ====================
# PyMovie Version 4.1.5
# source: C:\Users\aschw\Desktop\DvtiData\20251104_193750_408x310_G30dBD_20.0ms.adv
#
# Aperture photometry was used to extract the lightcurves
#
# lunar background: False
# yellow mask = default: False
#
# aperture name: target
# ____ aperture size: 41
# ____ x,y: (200, 168) at frame 3000
# ____ threshold: 790
# ____ def mask radius: 3.2
# ____ color: red
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 0
#
# aperture name: tracking
# ____ aperture size: 41
# ____ x,y: (200, 269) at frame 3000
# ____ threshold: 682
# ____ def mask radius: 3.2
# ____ color: yellow
# ____ joggable: True
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 1
#
# date at frame 0: 2025-11-04
#ACQUISITION-DELAY: 0.0
#ALTITUDE: 570.3
#AUTHOR: Andreas Schweizer
#BINNING-X: 4
#BINNING-Y: 4
#CAMERA-DRIVER-NAME: UVC
#CAMERA-FIRMWARE-VERSION: 1.3.3
#CAMERA-MODEL: DVTI+CAM
#CAMERA-SENSOR-INFO: Sony IMX430LLJ-C (9.2mm 1624x1240 4.5um CIS)
#CAMERA-SERIAL-NO: 109
#CAMERA-VENDOR-NAME: DVTI
#COMMENT: 
#DEC: 20.590156
#HEIGHT: 310
#INSTRUMENT: DVTI+CAM #109 FW 1.3.3, Sensor IMX430
#LATITUDE: 47.3418385
#LONGITUDE: 8.4728736
#OBJNAME: (189753) 2001 YS127 occ. TYC 1195-01065-1
#OBSERVER: Andreas Schweizer
#RA: 1.053888
#RECORDER-SOFTWARE: DvtiCamControl
#RECORDER-SOFTWARE-VERSION: 5.9.0-81
#TELESCOPE: Boren Simon
#WIDTH: 408
#
# Aperture photometry was used to extract the lightcurves
==================== end header lines ====================

No time step irregularities found.

timeDelta: 0.0199947 seconds per reading
timestamp error rate: 0.00%

Home directory: C:\Users\aschw\AppData\Local\Packages\PythonSoftwareFoundation.Python.3.10_qbz5n2kfra8p0\LocalCache\local-packages\Python310\site-packages\pyoteapp

We found C:\Users\aschw\Documents\model-examples already present. Adding any new examples ...
D zone selected: [1679, 1700]

R zone selected: [1703, 1722]

Locate a "D and R" event has been selected

Number of candidate solutions: 440 (using D/R region selections)

New solver results...

Integer (non-subframe) solution...
B:25650.02  A:299.11
in entryNum units: D: 1692  R: 1711

noise corr coefs: [1.00, 0.244, 0.0628, 0.0615]  (based on 2982 points)  sigmaB: 2661.71

noise corr coefs: [1.00, 0.241, 0.0704, 0.0608]  (based on 2981 points)  sigmaB: 2654.45

Subframe adjusted solution...
B:25653.73  A:-148.17
in entryNum units: D: 1692  R: 1711  D(subframe): 1692.3176  R(subframe): 1711.4359

in frameNum units: D: 1692  R: 1711  D(subframe): 1692.3176  R(subframe): 1711.4359

... end New solver results

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.0768
hiDbar   @ .68 ci:   0.0770
loDbar   @ .95 ci:  -0.1736
hiDbar   @ .95 ci:   0.1627
loDbar   @ .9973 ci:  -0.3301
hiDbar   @ .9973 ci:   0.3606

loDurBar @ .68 ci:  -0.1148
hiDurBar @ .68 ci:   0.1122
loDurBar @ .95 ci:  -0.2412
hiDurBar @ .95 ci:   0.2377
loDurBar @ .9973 ci:  -0.4216
hiDurBar @ .9973 ci:   0.4517

Timestamp validity check ...

From timestamps at D and R, calculated 19 reading blocks.  From reading blocks, calculated 19 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 25653.73  {+/- 48.62}  sigmaB: 2654.45

A: -148.17  {+/- 297.04}  sigmaA: 1264.38

magDrop report: percentDrop: 100.0  (magDrop cannot be calculated because A is negative)

DNR: 9.72

D: 1692.32 {+0.08,-0.08} (frame number)
D: [19:38:24.3304]  {+0.0015,-0.0015} seconds

R: 1711.44 {+0.08,-0.08} (frame number)
R: [19:38:24.7127]  {+0.0015,-0.0015} seconds

Duration (R - D): 19.1183 {+0.1135,-0.1135} readings
Duration (R - D): 0.3824 {+0.0023,-0.0023} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 25653.73  {+/- 97.24}  sigmaB: 2654.45

A: -148.17  {+/- 594.09}  sigmaA: 1264.38

magDrop report: percentDrop: 100.0  (magDrop cannot be calculated because A is negative)

DNR: 9.72

D: 1692.32 {+0.16,-0.17} (frame number)
D: [19:38:24.3304]  {+0.0033,-0.0035} seconds

R: 1711.44 {+0.17,-0.16} (frame number)
R: [19:38:24.7127]  {+0.0035,-0.0033} seconds

Duration (R - D): 19.1183 {+0.2395,-0.2395} readings
Duration (R - D): 0.3824 {+0.0048,-0.0048} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 25653.73  {+/- 145.86}  sigmaB: 2654.45

A: -148.17  {+/- 891.13}  sigmaA: 1264.38

magDrop report: percentDrop: 100.0  (magDrop cannot be calculated because A is negative)

DNR: 9.72

D: 1692.32 {+0.36,-0.33} (frame number)
D: [19:38:24.3304]  {+0.0072,-0.0066} seconds

R: 1711.44 {+0.33,-0.36} (frame number)
R: [19:38:24.7127]  {+0.0066,-0.0072} seconds

Duration (R - D): 19.1183 {+0.4367,-0.4367} readings
Duration (R - D): 0.3824 {+0.0087,-0.0087} seconds

=============== end 0.9973 containment interval report =============

D frame number: 1692.32
D: 0.6800 containment intervals:  {+/- 0.08} (readings)
D: 0.9500 containment intervals:  {+/- 0.17} (readings)
D: 0.9973 containment intervals:  {+/- 0.36} (readings)

R frame number: 1711.44
R: 0.6800 containment intervals:  {+/- 0.08} (readings)
R: 0.9500 containment intervals:  {+/- 0.17} (readings)
R: 0.9973 containment intervals:  {+/- 0.36} (readings)

Duration (R - D): 19.1183 readings
Duration: 0.6800 containment intervals:  {+/- 0.1135} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.2395} (readings)
Duration: 0.9973 containment intervals:  {+/- 0.4367} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.


The observed drop has an estimated 41.7 sigma level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 100.0  (magDrop cannot be calculated because A is negative)

DNR: 9.72

D time: [19:38:24.3304]
D: 0.6800 containment intervals:  {+/- 0.0015} seconds
D: 0.9500 containment intervals:  {+/- 0.0035} seconds
D: 0.9973 containment intervals:  {+/- 0.0072} seconds

R time: [19:38:24.7127]
R: 0.6800 containment intervals:  {+/- 0.0015} seconds
R: 0.9500 containment intervals:  {+/- 0.0035} seconds
R: 0.9973 containment intervals:  {+/- 0.0072} seconds

Duration (R - D): 0.3824 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0023} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0048} seconds
Duration: 0.9973 containment intervals:  {+/- 0.0087} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-target

fit metrics === noiseSigmaDistance: 81.3

fit metrics === time error bar: +/- 0.0035 seconds

fit metrics === DNR: 9.72  
fit metrics === B: 25653.73  A: -148.17 sigmaB: 2654.45  sigmaA: 1264.38
fit metrics === magDrop report: percentDrop: 100.0  (magDrop cannot be calculated because A is negative)

fit metrics === D frame number: 1692.3176

fit metrics === R frame number: 1711.4359

fit metrics === duration: 0.3823 seconds

fit metrics === D time: [19:38:24.3304]

fit metrics === R time: [19:38:24.7127]




All data points were selected

Data trimmed/selected using points: [1442, 1953]

